|  |  |  |  |
| --- | --- | --- | --- |
| **THE GoMog SERVICE LISTC:\DATAmog\allmorgan\goldenfrog2.jpg** |  |  |  |
| **[ENGINE AREA](file:///C%3A/DATAmog/allmorgan/GoMogServiceList.html%22%20%5Cl%20%22CARB_ENGINES)** | **DONE** |  |  |
| **Drain oil – replace oil filter – Fill up (All cars save Plus 8s *see below*)** | . |  |  |
| **Fill new oil filter -** [**replace old oil filter**](http://www.gomog.com/allmorgan/plus8oil.htm#Change) **- Drain & fill up. (Plus 8s only)** | . |  |  |
| **Replace spark plugs – check & adjust gap to engine's spec** | . |  |  |
| [**Examine old plugs for condition**](http://www.ngksparkplugs.com/tech_support/spark_plugs/faqs/faqread.asp) | . |  |  |
| [**Checking spark plug wires/leads & connectors**](https://www.youtube.com/watch?v=U27Gp_uQDLU) | . |  |  |
| **Check heater valve cable** | . |  |  |
| **Check fan belt tension and wear** [**Note for later Plus 8s**](http://www.gomog.com/allmorgan/plus8serpentinefanbelts.html) | **.** |  |  |
| **Check dynamo or alternator wiring** | **.** |  |  |
| **Check regulator and fuse box for corrosion (if applicable)** | **.** |  |  |
| **Check all engine mountings for bolt tightness and cracks in the rubber sections** | **.** |  |  |
| **Check slave cylinder leaks and clutch master cylinder fluid level (if hydraulic) (change both fluid every two years)** |  |  |  |
| **Check, lub and adjust clutch linkage and cable** | **.** |  |  |
| **Check, lub and adjust accelerator linkage and cable** |  |  |  |
| [**Check function of Inertia Switch**](http://www.gomog.com/allmorgan/DimDip.html#INERTIA) | . |  |  |
| [**Check engine earth (s) VERY carefully (both sides of the strap) for broken strands or a bad contact**](http://www.gomog.com/starter.htm#battery) | . |  |  |
| **Clean and dielectric grease earth strap(s) contact (s) on chassis** | . |  |  |
| . |  |  |  |
| . |  |  |  |