|  |  |
| --- | --- |
| **GoMoG SERVICE LISTC:\DATAmog\allmorgan\goldenfrog2.jpg** |  |
| **[REAR AXLE](http://www.gomog.com/allmorgan/gearindex.htm)** | DONE |
| [**Grease Salisbury Axle (pre-1995)**](http://www.gomog.com/allmorgan/axlefilling.html#Greasing) **(it is unnecessary to grease BTR axles)** | . |
| **Check level in Axle** |  |
| **Drain and replace oil (**[**Salisbury**](http://www.gomog.com/allmorgan/axlefilling.html#SALISBURY) **every 3000 miles)with a**[**BTR**](http://www.gomog.com/allmorgan/axlefilling.html#BTR) **check the level every 3000 miles and change fluid every 30,000 miles)**   | . |
| **Grease rear propshaft U-J nipple** | **.** |
| **Check propshaft to axle nuts for tightness** | . |
|  |  |
|  |  |
| **[REAR SUSPENSION](http://www.gomog.com/allmorgan/suspensionindex.html)** |  |
| **Check leaf springs for breaks** | **.** |
| [**Chain lube leaf springs**](http://www.gomog.com/allmorgan27.html#Leaf) | **.** |
| **Re-tighten U-bolts nyloc nuts or** [**stoffer nuts**](http://www.gomog.com/allmorgan/AXLEclunk.html) | . |
| **Check shock absorbers – check for leaks (or oil level on Armstrongs)** | **.** |
|  |  |