|  |  |
| --- | --- |
| .**GoMoG SERVICE LIST** |  |
| **REAR COMPARTMENT** | **DONE** |
| **Check and clean battery terminals and chassis connection** | **.** |
| **Apply petroleum jelly or dilectric grease to terminals and chassis connection point** | **.** |
| **Check battery acid level (if applicable)** | . |
| [**Check battery earth VERY carefully (both sides) for broken strands or a bad contact**](http://www.gomog.com/starter.htm#battery) | **.** |
| **Check play and grease rear zirk on prop shaft U-J** | . |
|  |  |
|  |  |
| **[REAR BRAKES](http://www.gomog.com/allmorgan/brakeindex.htm)** |  |
| [**Remove brake drums**](http://www.gomog.com/allmorgan/allmorgan45.html#REMOVAL) **–** [**check shoe wear**](http://www.gomog.com/brakes.html#Brake%20Pads%20and%20Brake) | **.** |
| **Check** [**slave cylinders**](http://www.gomog.com/allmorgan/brakes.html#Slave) **for leakage and/or gaiter/seal cracks** | **.** |
| **Clean and grease** [**hand brake mechanism**](http://www.gomog.com/allmorgan/handbrake.html) | **.** |
| **Clean and free** [**hand brake adjuster**](http://www.gomog.com/allmorgan/handbrake.html) **(pre-June 1993)** | **.** |
| **Check half shaft oil seal** | **.** |
| **Grease and re-pack half shaft bearings** | **.** |
| [**Check brake drum**](http://www.gomog.com/allmorgan/brakes.html#Remember)**. Clean and refit** | **.** |
| [**Adjust brake shoes**](http://www.gomog.com/allmorgan22.html#Adjustments) **(pre-June 1993)** | . |
| [**Adjust hand brake cable**](http://www.gomog.com//allmorgan/APBRAKES.html)**(post-June 1993)** | **,** |
| [**Safety Brake Watchpoint (post-June 1993)**](http://www.gomog.com//allmorgan/APBRAKES.html#SAFETY) |  |
| [**Check brake hoses and lines**](http://www.gomog.com/brakes.html#Hoses) | **.** |
| [**Bleed rear brakes**](http://www.gomog.com/allmorgan/bleeding.html) | **.** |
|  |  |
|  |  |