|  |  |
| --- | --- |
| **GoMoG SERVICE LISTC:\DATAmog\allmorgan\goldenfrog2.jpg** |  |
| **[COCKPIT](http://www.gomog.com/allmorgan/interiorindex.htm)** | DONE |
| **Check all fuses and relays** |  |
| **Check wiper blades – 1 drop of Vaseline oil on spindles** | **.** |
| **Grease windscreen wiper rack and pinions** | **.** |
| **Grease thrust bearing sleeve (Series I, early Plus 4 and Moss box Plus 8s)** | **.** |
| **Grease pedal set and throttle pedal** | **.** |
| **Check pedal rubbers, change if required** | **.** |
| **Grease hand brake ratchet and cable** | **.** |
| **Check gearbox level (change every 10,000 miles)** | **.** |
| **Check play and grease zirk on front propshaft UJ.** [**Omit the one on the propshaft.**](http://www.gomog.com/allmorgan/axlefilling.html#WATCHPOINT) | **.** |
| **Check spline on prop shaft (early cars)** | **.** |
| **Check propshaft to gearbox nuts for tightness** |  |
| **Lube seat sliders *Use a greaseless spray lubricant*** | **.** |
| [**Clean and recondition leather**](http://www.gomog.com/allmorgan/leatherhelp.html) | **.** |
| **Check all electrics and gauges are functioning correctly**[**Instruments**](http://www.gomog.com/allmorgan/instrumentindex.html) | . |
| **Lube bonnet hinge and catches (Vaseline oil)** | **.** |
| **Lube door hinges and catches** [**Metal Section 3**](http://www.gomog.com/allmorgan/metalindex.htm) | . |
| . |  |