|  |
| --- |
| **GoMoG SERVICE LISTC:\DATAmog\allmorgan\goldenfrog2.jpg** |
|  |  |
| **[COOLANT SYSTEM](http://www.gomog.com/allmorgan/coolingindex.htm)** | **DONE** |
|  |  |
| [**Check rad hoses for correct firmness, cracks or rubbing**](http://www.gomog.com/allmorgan/Hoses%26Clamps.html) | **.** |
| **Check rad for leaks or rubbing** | **.** |
| [**Check coolant level**](http://www.gomog.com/allmorgan/TANKS.html) | **.** |
| [**Test coolant quality**](http://www.gomog.com/allmorgan/voltagestabilizer.html#COOLANT) | **.** |
| **Change** [**coolant**](http://www.gomog.com/allmorgan/coolantcolors.html)**.** [**Flush**](http://www.gomog.com/allmorgan14.html#Flushing%20a%20Your%20Radiator) **and change every two years** | **.** |
| [**Check rad cap for leaks when hot**](http://www.gomog.com/allmorgan/RadCapsMorgan.jpg) | . |
| [**Test Coolant for electricity**](http://www.gomog.com/allmorgan/voltagestabilizer.html#TESTING)**(very important for alloy engines and rads)** | . |
| **Check fan function and the direction the blades are turning** [**Cooling Section 6**](http://www.gomog.com/allmorgan/coolingindex.htm) | . |
| . |  |