|  |  |
| --- | --- |
| .**GoMoG SERVICE LIST**. | DONE |
| **[DISTRIBUTOR IGNITIONS](http://www.gomog.com/allmorgan/ignitionindex.html)** |  |
| **Check distributor cap – contact points for cracked Bakelite** [**Ignition Index**](http://www.gomog.com/allmorgan/ignitionindex.html) | **.** |
| **Check condition of rotor** [**Ignition Index**](http://www.gomog.com/allmorgan/ignitionindex.html) | . |
| **Check wear on distributor shaft.  (especially Kent engine)** | **.** |
| **Check condition of vacuum auto advance pipe** | . |
| **Check function of vacuum advance (with strobe)** | . |
| **Check dynamic advance  (with strobe)** | **.** |
| **Check throttle cable – adjust tension if necessary** | **.** |
| [**Change (or clean with K&Ns) the air filter (s)**](http://www.bobistheoilguy.com/airfilter/airtest1.htm) | . |
| **Change contact breaker – adjust points** |  |
| **Check dwell angle (if needed)** |  |
| . |  |