|  |  |
| --- | --- |
| **GoMoG Service List** | |
| [**FRONT SUSPENSION AREA**](http://www.gomog.com/allmorgan/suspensionindex.html) | **DONE** |
| [**Check play in bushes**](http://www.gomog.com/allmorgan2.html#Checking) | . |
| **Clean bottom part –** [**check for rust**](http://www.gomog.com/allmorgan6.html#primary) **on kingpin  (switch to** [**hardchromes**](http://www.gomog.com/allmorgan6.html#Hard)**)** | . |
| [**Check bottom nyloc nut and base plate bolts or tightness**](http://www.gomog.com/allmorgan/lowerplayebolts.jpg) | . |
| **Check** [**one-shot**](http://www.gomog.com/allmorgan6.html#One) **lube bolt – brush clean and lube the one shot union  (with WD40) (pre-2002)** | . |
| **Check** [**one shot**](http://www.gomog.com/allmorgan6.html#One) **pipe (pre-2002)** | . |
| **Check the wing/side-light nuts for tightness** | . |
| [**Check wing stay**](http://www.gomog.com/allmorgan/wingstays.html) **(replace them with your own if you have a post 2001 version)** |  |
| **Clear vent hole at bottom of top tube of slider *(yes there is one at the rear)*** | . |
| [**Grease bushes according to year**](http://www.gomog.com/allmorgan9.html#Dynamics) | . |
| [**Change damper blade shims**](http://www.gomog.com/allmorgan6.html#Damper) **– turn damper blades over – grease (pre-2008)** | . |
| **Check shocks for proper function.  *(article needed!)*** | . |
| **Check front indicator lights**[**Electrical Index Section 11**](http://www.gomog.com/allmorgan/electricindex.htm) |  |
| **Check front parking lights**[**Electrical Index Section 11**](http://www.gomog.com/allmorgan/electricindex.htm) |  |
| [**Check wing lights**](http://www.gomog.com/allmorgan/wingstays.html#WATCHPOINT) |  |
| **Check Hazard Lights**[**Electrical Index Section 11**](http://www.gomog.com/allmorgan/electricindex.htm) |  |
| [**Check Headlamp Alignment**](http://www.gomog.com/other.html#Adjusting) |  |
| [**Check horn (s)**](http://www.gomog.com/allmorgan29.html#HORNS) |  |
| **Check bumper bolts,  attachments and support bolts** |  |
|  |  |
|  |  |